
Product Name: Enova DGX 8/16/32/64 Enclosures

=========== ======================  ======================
FG #        Name                    Description
=========== ======================  ======================
FG1058-08   AVS-ENOVADGX8-ENC       Enova DGX 8 Enclosure
FG1058-16   AVS-ENOVADGX16-ENC      Enova DGX 16 Enclosure
FG1059-32   AVS-ENOVADGX32-ENC      Enova DGX 32 Enclosure
FG1059-33   AVS-ENOVADGX32-ENC-A    Enova DGX 32 Enclosure
FG1060-08   DGX8-ENC                Enova DGX 8 Enclosure
FG1060-16   DGX16-ENC               Enova DGX 16 Enclosure
FG1060-32   DGX32-ENC-A             Enova DGX 32 Enclosure
FG1060-64   DGX64-ENC               Enova DGX 64 Enclosure


*****************IMPORTANT********************************
 If sending this kit to a DGX 8/16/32 with
 v1.6.5.13 (or earlier), you MUST FIRST send
 the following kit to the Enova DGX enclosure:
 "LOAD_BEFORE_SENDING_DGX_KIT.kit"
 (This takes around 1 minute to complete)
**********************************************************


IMPORTANT NOTE ABOUT TIME REQUIRED TO UPGRADE:
  See the Programming Information section in this
  read me for an explanation of how to know when
  the upgrade is complete as well as estimates of
  the time required for the update to successfully
  upgrade.  Ignoring this information could cause
  your upgrade to fail to complete.



Current Firmware Version: 2.2.12-1
Build Date: 2017-11-22

Website Availability: EnovaDGX_2.2.12-1.kit
Device Id: 5002

EnovaDGX KIT file 2.2.12-1 contains these firmware images:

* Indicates changes since v2.2.12

- MCPU 8 NI-Series          v2.6.2.2
- MCPU 16 NI-Series         v2.6.2.2
- MCPU 32 NI-Series         v2.6.2.2
- MCPU 8 NX-Series          v2.8.2.4
- MCPU 16 NX-Series         v2.8.2.4
- MCPU 32 NX-Series         v2.8.2.4
- MCPU 64 NX-Series         v2.8.2.4
- Power BCPU 8 NI-Series    v2.2.2.1
- Power BCPU 16 NI-Series   v2.2.2.1
- Power BCPU 32 NI-Series   v2.2.2.1
- Power BCPU Nx-Series      v2.4.1.6
- DGX Center Board          v2.0.4.3
- SC Fiber Input            v2.0.0.6
- SC Fiber Output           v2.0.1.2
- DVI/HDMI Input            v1.4.4.5*
- DVI/HDMI Output           v1.4.3.3
- DXLink Input              v1.4.6.6*
- DXLink Output             v1.4.5.2*
- DGX AIE Board             v1.0.0.4
- DGX64 AIE Board           v2.0.1.1
- 6p switch                 v1.0.2.1
- 24p Config                v1.2.1.1
- 24p ext Board             v1.0.0.2
- DXLink Rx FW              v3.0.6.0
- DXLink Tx FW              v3.0.6.0
- DXLink Fiber Fw           v1.0.1.4
- Output Scaler             v1.17
- SRM File                  v1.0.5.1

- Integrated App            v1.2.1.15




----------------------------------------------------------
Prerequisites
----------------------------------------------------------

- NetLinx Studio v4.0 or later

- NI Series Master Firmware v4.2.395 or later
- NX Series (X200) Master Firmware v1.4.90 or later

Endpoints should have the following versions to be compatible

- DXLink DX-TX v1.8.28 or later
- DXLink DX-RX v1.13.34 or later
- DXLink DXF-TX v1.4.12 or later
- DXLink DXF-RX v1.4.17 or later
- Solecis SDX-X10-DX v1.4.9 or later

NOTE: Older TX & RX firmware versions (1.6.xx & 1.9.xx)
are specifically not supported with this DGX kit fw

= = = = = = = = = = = = = = = = = = = = = = = = = = = = = =
! ! ! ! ! ! ! ! ! I M P O R T  A N T ! ! !  ! ! ! ! ! ! ! !
= = = = = = = = = = = = = = = = = = = = = = = = = = = = = =
NOTE: This update is only required for an existing Enova DGX
system (running v2.0.2.2 or earlier) IF new DGX 100 series
I/O cards OR endpoints are being added to that system and the
user does not wish to downgrade the new cards or endpoints
to match their existing system firmware. Mixed rev systems
are NOT supported.

It is recommended to update the DGX enclosre/cards first and
then update any attached endpoints to the compatible versions
listed above.


----------------------------------------------------------
Changes in this release
----------------------------------------------------------

HDMI Input
 - Corrected issue where AIE state may not report correctly

HDMI/DVI Output boards
 - Fixed issue where upstream instability (hotplugs, garbage
   video, etc.) could result in HDMI outputs encountering
   various video artifacts (sawtooth, posterization, venetian
   blinds, black video, etc.)
 - Fixed issue where upstream instabiltiy could cause
   extracted audio from AIE outputs to drop unexpectedly

DXLink Input
 - Fixed issue where async notifications from upstream
   Solecis 2K switchers were being blocked
 - Fixed issue with HDCP compliance setting when using a
   4K WP and the source is disconnected or asleep
 - Modify DGX_SHELL>channel command to show freerun res/ref
   when no signal present
 - Updated firmware to support alternate flash memory parts
   NOTE: Boards using these new parts will not function with
   firmware earlier than v1.4.6.5 - Do not roll back.

DXLink Output
 - Fixed issue where hotplugging Fiber Rx can cause DXLink
   output card to reboot

----------------------------------------------------------
Known Issues
----------------------------------------------------------
- A wait of 15seconds is required when Hot Swapping DGX
  I/O boards


- DGX Configuration Software
  The Scaler tabs may not accurately reflect current
  settings with this revision of the output cards but
  the scaler settings are being applied when set.

      The DGX Config Software has not been tested with any
      non-English versions of Windows XP or Windows 7.

- DXLink Tx Fw v3.0.6.0
     The "show stats" DGX Shell command (or "show vs100
     stats" from the DXLINK TX/RX telnet command) may
     report some cable lengths approaching 100m as 255m.
     This is a reporting limitation imposed by the chip mfr
     for TX v3.0.6.0 and does not affect the functionality.
     This applies to any DGX or DVX DXLink output, or any
     DXLink TX/MFTX module or wallplate using this version.

- DO NOT USE THE "DGX_SHELL>reboot" command with older
  ENOVA DGX 8/16/32 Enclosures with Power-One Power
  Supplies that have the new CPU with NX-Series Master.
  This WILL cause the cards to not power up and REQUIRE a
  hard power cycle of the cage. Power-One supplies may be
  identified in the ~scr6v3! or with the
  "DGX_SHELL>power INFO" command by model number:
  e.g. model: FNP850-12ARG (Power-One Supply)


----------------------------------------------------------
Programming Information
----------------------------------------------------------
-  If sending this kit to a DGX 8/16/32 with v1.6.5.13 or
   earlier, you MUST FIRST send the following kit to the
   Enova DGX enclosure: "LOAD_BEFORE_SENDING_DGX_KIT.kit"
   This takes around 1 minute to complete. Once completed,
   refresh the System Online Tree and expand the 5002
   device to verify that the Integrated Device version is
   now at v1.2.1.15 - Then send this DGX kit to complete
   the system upgrade

- Upgrade time may take up to 2 hours.

- The only reliable way to monitor the upgrade is to jump
  directly to the upgrade status page with the url:
  http://master_ipAddr/web/upgrade/systemUpgradeStatus.xml
  before initiating the KIT upgrade to monitor the runtime
  upgrade status.

- It is recommended that you disable any program running
  on the DGX or that you disable any program using the
  Enova DGX BCSTunnel service before initiating the Enova
  DGX KIT firmware upgrade.

- It is also recommended that you disconnect/disable any
  control system using the external serial connection(s)
  during any KIT file upgrades.

- After the Upgrade Status page has indicated that the
  Enova DGX firmware upgrade was successful and device
  5002 has come back online, it is recommended that you
  power cycle the DGX to insure all endpoint devices come
  back online properly.

- New HDMI/DVI Input boards will only work with v1.0.6.4
  image or greater (v2.0.0.10 DGX KIT) or greater due to
  hardware design change. It can be identified in the shell
  "show" command with a hardware ID of 1 (HW_ID 0x1).

- New DXLink Fiber Input/Output Simplex Boards will
  not be compatible with v1.2.0.x DXLink images or older.
  Enova DGX KIT v2.0.0.8 or older will fail to load with
  these boards present in the system.
